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	DIFFERENTIAL SCANNING CALORIMETER 
	Application example: 
Measurement of PET granulate
Technical specification
Temperature range: -150 up to 600°C 
Heating and cooling rates:0,001 up to 1000 K/min
Temperature accuracy: +/- 0,2 K
Temperature precision: +/- 0,02K
Digital resolution:16.8 million points
Resolution:0,03 µW
atmospheres: inert, oxidizing (static, dynamic)
Measuring range:+/-2,5 up to +/-250 mW
Calibration materials: included
Calibration: recommended 6-month interval
Documentation:
· CE marking and declaration conformity
· Documents for the Installation and Operational Qualification (IQ / OQ)
· Functional Specification - Design Qualification (DQ) and others relevant document
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