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	1
	X-RAY DIFFRACTION (XRD)
	Application
Used in Cement, Material Properties, Minerals & Mining, Oil & Gas
Technical specification
Goniometer Theta / Theta-Sample is always horizontal and cannot fall off during measurement
Angular accuracy: Exact peak positions better 0.02°2Theta over entire measurement range, Traceable by included corundum reference
Sample stages: Single or 6-position, rotating
Setup: Plug’n Analyze- No Installation, no alignment, no instrument configuration
110 -220 V, 50 - 60 Hz -All domestic wall sockets supported
Integrated PC / monitor- Little space requirements
Internal cooling-No water supply needed
Weight: 95 kg, 210 lbs 
Size: (H W D )61x60x70 cm (42.02″x23.62″x27.56″)
Documentation:
· CE marking and declaration conformity
· Documents for the Installation and Operational Qualification (IQ / OQ)
· Functional Specification - Design Qualification (DQ) and others relevant document
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