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	X-RAY FLUORESCENCE ANALYZER
	Features
 Speedy, Small, Simple, Smart, Safe
Application
Non-destructive Thickness and Composition Analysis of Coatings on Steel
Fast, easy and safe control of Zn-Ni galvanization baths
Solid Waste Combustors and Incinerators in Solid Waste Management and Remediation Services
Technical specification
Basic Items
Principle: Energy dispersive X-ray fluorescence spectrometry
Target application: RoHS, ELV, Halogen Free
Meas. Elements: 13Al - 92U
Sample type: Solid, Liquid, Powder
X-ray generator
X-ray tube: Max 50kV, 0.2mA
X-ray irradiation size: 1.2mm, 3mm, 7mm (Automatic switching)
X-ray primary filter: 4 types (Automatic switching)
Detector
Type: SDD (Silicon Drift Detector)
Signal processor: Digital pulse processor
Sample chamber
 Atmosphere: Air
Sample observation: CCD camera
Utility
Operation: PC 
Power supply: AC adapter (100-240V, 50/60Hz)
Documentation:
· CE marking and declaration conformity
· Documents for the Installation and Operational Qualification (IQ / OQ)
· Functional Specification - Design Qualification (DQ) and others relevant document
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