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	X-RAY FLUORESCENCE ANALYZER
	Features
Speedy, Small, Simple, Smart, Safe
Application
Non-destructive Thickness and Composition Analysis of Coatings on Steel
Solid Waste Combustors and Incinerators in Solid Waste Management and Remediation Services
analysis for the Electronics Industry
Technical specification
Basic Items
Principle: Energy dispersive X-ray fluorescence spectrometry
Target application: RoHS, ELV, Halogen Free
Meas. Elements: 13Al - 92U
Sample type: Solid, Liquid, Powder
X-ray generator
X-ray tube: Max 50kV, 0.2mA
X-ray irradiation size: 1.2mm, 3mm, 7mm (Automatic switching)
X-ray primary filter: 4 types (Automatic switching) 
Detector
 Type: SDD (Silicon Drift Detector)
Signal processor: Digital pulse processor
Sample chamber	
Atmosphere: Air
Sample observation: CCD camera
Chamber size: 460 x 360 x 150 mm [W x D x H]
Utility	
Operation: PC 
Power supply: 100-240V, 50/60Hz
Dimensions: 590 x 590 x 400 mm [W x D x H]
Weight: 60 kg
Documentation:
· CE marking and declaration conformity
· Documents for the Installation and Operational Qualification (IQ / OQ)
· Functional Specification - Design Qualification (DQ) and others relevant document
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