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	1
	PULSED LASER AND LED LIGHT SOURCES
	Features
· The widest range of interchangeable heads
· Short optical pulses from <50ps optical FWHM
· Repetition rated up to 100MHz
· Wavelengths from 250nm to NIR
· No additional optimization sources required in normal use
· Diode operating features full accessible for advanced applications
Technical specification
Repetition rates:10kHz,20kHz,50kHz,100kHz,250kHz,500kHz,1MHz,2MHz,4MHz,
8MHz,10MHz,16MHz,20MHz,25MHz, 50MHz,80MHz,100MHz or trigger input (single -shot to 50MHz) subject to attached head 
Trigger input: pulse amplitude+0.5V to +5V trigger threshold software programmable from+0.2V to 2V 
Interlock:2-pin connector. contacts must be short-circulated to enable emission
Connection to head: 1.5m cable 
User Interface: LCD display (stand-alone operation) or software (PC control)
PC interface: USB 2.0 with integral hub for downstream connection to other USB peripherals
Power requirement:90V to 260V AC ,50/60Hz, 100VA
Operating temperature: +15°C to +30°C (ambient)
Weight &dimension :3.1kg 234*255*92mm 
Documentation:
· CE marking and declaration conformity
· Documents for the Installation and Operational Qualification (IQ / OQ)
· Functional Specification - Design Qualification (DQ) and others relevant document
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