	Item No.
	Item Name
	Technical Specifications
	Unit of 
Measurement
	Quantity

	1
	KOH MONITOR
	Features
· Wide range measurement
    Concentration: 0 - 20%, Conductivity: 0 - 1000 mS/cm
· High precision
· PFA Sensor
 Technical specification
Target of measurement	KOH
Measurement range: Concentration: 0 - 20%, Conductivity: 0 - 1000mS/cm
Repeatability: Within +/- 0.5%R.D. or within 0.005wt% whichever is higher (Temperature variation less than +/- 0.5℃, using equivalent input for conductivity)
Linearity: Within +/- 0.5%R.D. or within 0.005wt% whichever is higher (Temperature variation less than +/- 0.5℃, using equivalent input for conductivity)
Transmission output: Number of output: 4
Contact output	Outputs: 5 points
Communication output	RS-485
Power supply: 24V DC +/- 10% 10W
Documentation:
1. CE marking and declaration conformity
1. Documents for the Installation and Operational Qualification (IQ / OQ)
1. Functional Specification - Design Qualification (DQ) and others relevant document
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