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	1
	MOISTURE ANALYZERS
	Description
Outstanding Performance, Flexible Configuration and Reliable Results
Application
Percent Moisture Determination, Percent Solid Determination, Weighing
Features
Glass-less infrared heating increases efficiency for faster results.
User-friendly touch-button design for easy operation.
Compact design suits any workspace
Technical specification
Maximum Capacity: 110 g
Readability Moisture Content: 10 mg/0.1%
Pan Size: 3.5 in (90 mm)
Display: Backlit liquid crystal display (LCD)
Operation: Power cord (included)
Communication: RS232 (included)
Construction: Infrared heat source, ABS housing, metal pan support, metal pan handler, in-use cover
Design Features: 3 shut off criteria (manual, timed or auto), 1 standard heating profile, 50° to 160° C heating range (5° C increments)
Documentation:
1. CE marking and declaration conformity
1. Documents for the Installation and Operational Qualification (IQ / OQ)
1. Functional Specification - Design Qualification (DQ) and others relevant document
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