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	1
	Dissolved Oxygen (DO) Meter
	Description
High-Performance, Low-Maintenance Dissolved Oxygen (DO) Meter with Optical Technology for Accurate Measurements
Application
Field and lab Dissolved Oxygen measurement
Features
· Large backlit LCD screen provides easy to read results - even in low light environments. Ideal for secure field use with a meter stand, wrist strap and durable IP54 housing.
· Optical DO probe requires minimal maintenance and offers immediate measurement readings. No warm up or sample preparation needed.
· The 99-measurement library stores data for future reference and allows for easy one-touch recall of the last calibration data.
Technical specification
Measurement Range: 0.00 – 20.0 mg/L(ppm);0 – 50°C
Accuracy: ±0.2 mg/L(<8 mg/L) or ±0.3 mg/L(8~20 mg/L);±0.3 °C
Measurement Resolution: 0.01 mg/L;0.1%;0.1 °C
Display: Backlit Color Liquid Crystal Display (LCD)
Operation: 4 AAA batteries (included)
Construction: ABS Housing
Design Features: 99 measurement memory, last calibration data recall, auto barometric pressure measurement, auto temperature compensation with manual salinity compensation
Documentation:
· CE marking and declaration conformity
· Documents for the Installation and Operational Qualification (IQ / OQ)
· Functional Specification - Design Qualification (DQ) and others relevant document
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