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	1
	Portable conductivity meter
	Description
Convenient Portable Conductivity Meter
Applications
Conductivity, total dissolved solids (TDS) measurement
Features
· Easy-to-use and accurate with a simple calibration process, automatic temperature compensation and fast results.
· Four-pole linear electrode with temperature sensor safeguards the unit from polarization and pollution effects to ensure accurate readings.
· The 30-measurement library stores data for future reference and allows the user to easily recall the last calibration data with one quick touch.
Technical specification
Measurement Range: 00.0 μS/cm – 199.9 mS/cm;0 – 100°C;0.1 mg/L – 199.9 g/L (TDS)
Measurement Resolution: 0.1 °C;0.01 μS/cm;0.1 mg/L
Display: Liquid crystal display (LCD)
Operation: 4 AAA batteries (included)
Construction: ABS housing, wrist strap
Design Features: Automatic temperature compensation, adjustable temperature coefficient
Documentation:
· CE marking and declaration conformity
· Documents for the Installation and Operational Qualification (IQ / OQ)
· Functional Specification - Design Qualification (DQ) and others relevant document
	pcs
	1



