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	1
	PH Meter
	Features
Extremely easy to use. It has a compact, portable design and is water resistant (IP67), so it can be cleaned under running water and submersed into water without any negative effects. It has an Automatic Temperature Compensation mechanism that function from 0 to 50°C.
Application
food and beverage production control, brewing and fermentation, soil and hydroponics, cutting oils, alkali washing liquids, and other soluble solutions.
Technical specification
Range	0.0 to 14.0pH
Resolution: 0.1pH
Accuracy: ± 0.1pH (2.0 to 12.0pH)
Temperature compensation: 0.0 to 50.0°C
Power Supply: Watch battery (LR44) × 4
Included Articles
Accessories
· Standard calibration solution pH 4.01 
· Standard calibration solution pH 7.00 
· Standard calibration solution pH 10.01 
Documentation
· CE marking and declaration conformity
· Documents for the Installation and Operational Qualification (IQ / OQ)
· Functional Specification - Design Qualification (DQ) and others relevant document
	pcs
	1



