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	1
	Benchtop PH meter
	Description
An Advanced, Research-Grade Benchtop pH Meter Offering Accurate, Repeatable Results
Application
pH, oxidation-reduction potential (ORP) with Temperature Measurements
Features
A 1000-item memory and password management for GLP documentation. Provides connectivity and data output capabilities with RS232 and USB interface.
Equipped with a 6.5-inch large LCD display and a touch keypad, offers a simple and precise control experience
Technical specification
Measurement Range
-2.000 – 20.000 pH;-10.0 °C – 125.0 °C;-2000.00 – +2000.00 mV
Measurement Resolution
0.1 mV;0.1 °C;0.001 pH
Accuracy
±0.3 mV;± 0.002 pH;±0.3 °C
Display: 6.5" Segment & Dot matrix LCD with backlight
Operation: Capacitive touch, ABS top housing, standalone electrode holder
Communication: RS232, USB Device (included), GLP/GMP data output with real-time clock
Construction: AC adapter (included)
Design Features: i-Steward, 3 endpoint modes, calibration due alarm, 1,000 measurement memory, ten most recent calibrations, password management
Documentation
· CE marking and declaration conformity
· Documents for the Installation and Operational Qualification (IQ / OQ)
· Functional Specification - Design Qualification (DQ) and others relevant document
	pcs
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