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	1
	WINE REFRACTOMETER
	Technical specification
Scale: T.A.1990
Range: 0.0 to 26.0%
Accuracy: ± 0.2%
Temperature compensation: 10 to 40°C
Sample Volume: 2 to 3 drops
Measurement Time: About 3 seconds
Power Supply: 2 × AAA Batteries
Battery Life: About 11,000 measurements
Dimensions & Weight: 5.5 × 3.1 × 10.9cm 100g (main unit only)
Included Articles
Accessories
· PAL-CASE 
· STRAP 
· Battery Case Cover With O-Ring 
· USB Battery Charger 
Documentation:
· CE marking and declaration conformity
· Documents for the Installation and Operational Qualification (IQ / OQ)
· Functional Specification - Design Qualification (DQ) and others relevant document
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