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	1
	3D X-RAY MICROSCOPY (XRM)
	Application
Additive manufacturing
Fibers and composites
Geology
Technical specification
X-ray source: 20-160 kV, 16 W max.
X-ray detector: 6 Mp active pixel flat-panel, 11 Mp large format cooled CCD, 11 Mp mid format cooled CCD, 8 Mp hi-res cooled CCD
Image Formats: Up to 8000 x 8000 x 2300 pixels after a single scan
Resolution: 60 nm smallest pixel size, <500 nm low-contrast resolution (10% MTF)
Positioning Accuracy: <50 nm for rotation, Anti-vibration granite platform with pneumatic leveling
Maximum Object Size: 300 mm in diameter (140 mm scanning size), 400 mm in length, Maximum object weight 20 kg
Dimensions: W 1800 mm x D 950 mm x H 1680 mm
Weight: 1500 kg
Documentation:
· CE marking and declaration conformity
· Documents for the Installation and Operational Qualification (IQ / OQ)
· Functional Specification - Design Qualification (DQ) and others relevant document
	Pcs
	1



