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	1
	MOISTURE ANALYZERS
	Description
Simple Operation. Precise Results.
Applications
Percent Moisture Determination, Percent Moisture Regain Determination, Percent Solid Determination, Weighing
Features
Halogen heating increases efficiency for faster results
Intuitive touchscreen menu offers step-by-step guidance for any application
Tool-free cleaning for easy maintenance.
Technical specification
Maximum Capacity: 90 g
Readability Moisture Content: 1 mg/0.01%
Pan Size: 90 mm
Display: 4.3" TFT color touchscreen display
Operation: Power cord (included)
Communication: RS232 with GLP/GMP data output, USB Host and USB Device (included)
Construction: Metal base, ABS top housing, halogen heat source, stainless steel pan support, stainless steel pan handler, in-use cover
Documentation:
1. CE marking and declaration conformity
1. Documents for the Installation and Operational Qualification (IQ / OQ)
1. Functional Specification - Design Qualification (DQ) and others relevant document
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