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	1
	PORTABLE PH METER
	Description
Durable, Waterproof Battery-Operated pH Meters Ideal for Field Testing
Application
pH, Oxidation-Reduction Potential (ORP) measurement
Features
Rechargeable lithium battery provides 40 hours of uninterrupted use and more than 300 charge cycles - eliminating the need to change out batteries often.
Technical specification
Measurement Range: -5 °C – 110 °C;-2.00 – 16.00 pH;-1999 – 1999 mV
Accuracy: ±0.5 °C;±1 mV;±0.01 pH
Measurement Resolution: 0.1 °C;0.01 pH;1 mV
Display: Backlit Liquid Crystal Display (LCD)
Operation: Rechargeable lithium battery
Communication: Built-in micro-USB port
Construction: IP67 waterproof plastic housing, IP67 probes, rubber cover
Design Features: Data storage of up to 1000 items
Documentation:
· CE marking and declaration conformity
· Documents for the Installation and Operational Qualification (IQ / OQ)
· Functional Specification - Design Qualification (DQ) and others relevant document
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